SEDAI 2020.05 [2020.05.18]
- System updates:
	* New Sedai Shell and Config with SDL support;
	* Linux kernel update to ver. 4.14.74;	
	* Samba 4.11.6 (preconfigured as sedai sharing);
	* OpenSSH 8.1p1 (preconfigure with root access);
- Emulators:
    * LinApple 2 emulator for Apple ][ and Apple //e emulation (NEW);
    * uae4arm-rpi with CAPSimage support;
    * Atari800 4.2.0;
    * Basilisk II (no updates);
    * DOSBox 0.74-3;
    * Fuse 1.5.7 with libspectrum 1.4.4 (no updates);
    * Hatari 2.2.1 with CAPSimage support;
    * openMSX 0.15.0 with libTheora for laserdisc support (no updates);
    * Vice 3.4 with SDL and FFMPEG;
    * ZEsarUX 8.1.
- Removed emulators:	
    * Amiberry;


--------------------------


SEDAI 0.1.105 [2019.03.16]
- System updates:
	* Linux kernel update to ver. 4.14.74;	
	* Samba 4.9.4;
	* OpenSSH 7.9;
- Emulators:
	* Amiberry 2.24;
	* Atari800 4.0.0 (no updates);
	* Basilisk II (no updates);
	* DOSBox 0.74-2 (instead of FastDOSBox);
	* Fuse 1.5.7 (Free Unix Spectrum Emulator) with libspectrum 1.4.4;
	* Hatari 2.2.0;
	* openMSX 0.15.0 with libTheora for laserdisc support;
	* Vice 3.3 with SDL2 and FFMPEG;
	* ZEsarUX 7.1 final.
	

--------------------------
	

SEDAI 0.1.105 [2018.08.17]

BUGS FIXED:
- System:
	* some missed files;
- SedaiConfig:
	* unable to resize user partition in some conditions;
	* unable to start some emulators;
	* other minor bugs;
- SedaiShell:
	* unable to run some emulators to boot time;
	* use 'dispmanx' driver instead of 'fbcon' running openMSX;
	* other minor bugs;
- SedaiStart:
	* minor bugs;


--------------------------

	
SEDAI 0.1.103 [2018.08.16]


WHAT'S NEW
- System:
	* SedaiConfig for system auto-configuration;
	* SedaiShell graphical user interface;
	* Automatic 3th partition resizing and initialisation;
	* All configuration files moved in the 3th partition;
	* All emulated computer models are now supported;
	* Linux kernel updated to ver. 4.14.29;
	* Midnight Commander 4.8.20;
	* Samba 4.8.1 (SMB) for partition sharing;
	* OpenSSH 7.7 client;	
	* Support for many keyboard layouts;
- Emulators:
	* Amiberry 2.19 with SDL2;
	* Atari800 4.0.0;
    * Basilisk II;
    * FastDOSBox 1.6;
	* Free Unix Spectrum Emulator (Fuse) 1.5.5 and libspectrum 1.4.3;
	* Vice 3.2 with SDL2;	
	* ZEsarUX 7.1;	
- Development:
	* Added xa high-speed, two-pass portable cross-assembler. 
	  It understands mnemonics and generates code for NMOS 6502s 
      (such as 6502A, 6504, 6507, 6510, 7501, 8500, 8501, 8502 ...), 
	  CMOS 6502s (65C02 and Rockwell R65C02) and the 65C816. 
	  (https://www.floodgap.com/retrotech/xa/);

	  
NOT UPDATED
	- Hatari 0.9.9.1;
	- openMSX 0.14.0;
	 

--------------------------


TODO
- System:
	* More keyboard layouts;	
	* OpenSSH 7.7 server;
- All emulators: 
	* debug and general setup optimisation;
	* video output optimisation (both HDMI and composite);
	* support for original keyboards trought open source HID hardware;
	* more development tools for emulated platform;
- Fuse and ZEsarUX: add Arcade Game Designer 
  (https://jonathan-cauldwell.itch.io/arcade-game-designer);
- Olimex OLinuXino A64 porting;
- Pine Pine64/Rock64 porting;
- Asus Thinker Board porting;
- x86/x86-64/amd64 porting; 


SETUP
1) Unzip and flash the image on a microSD. 
   We suggest to use Etcher from https://etcher.io/.
2) Insert the microSD in you Raspberry Pi 2B, 3B, 3B+ or CM3 dev. board and turn 
   on the unit;
3) Select your keyboard layout when asked;
4) Select your emulator and press F2 to run it at boot time.


MINIMUM REQUIREMENTS
- Raspberry Pi mod. 2B, mod. 3B or 3B+ or CM3 recommended;
- USB keyboard and mouse;
- microSD 2GB.


WARNING
- Sedai Linux forces the Raspberry Pi to run at 1.2 GHz clock. No overclock is 
  applied, but use of heatsink is suggested to avoid damages on the long run.
- This distribution is a prototype, is incomplete and could be changed without 
  notice.
- Users of this ditribution do so at their own risk.
